**SCRAM Fit Adjustment**

**1. Complete the Bracelet Maintenance Wizard**

To complete the Bracelet Maintenance wizard:

a. Access the client’s Equipment page.

b. Click the Maintenance link.

c. Select the **Fit Adjusted** check box.

d. Click the **Finish** button.

The bracelet re-initialization, which must be performed each time the bracelet is

removed, will begin the next time that the bracelet communicates with SCRAMNET.

**2. Remove SCRAM CAM Bracelet Tamper Clips for Fit Adjustment**

To remove the bracelet:

a. Place the shear cutter on the center line where the two pieces of the tamper clip meet.

b. Press down firmly with one point of the shear cutter until the point breaks through the

plastic.

c. Press down firmly with the other point of the shear cutter until that point breaks through

the plastic.

d. Squeeze the shear-cutter handles until the plastic center breaks and the two pieces

separate from the buckle cover.

e. Using the T10 screwdriver, loosen the two retaining screws.

f. Perform your fit adjustment, place the bracelet no more than an index finger above the right or left ankle with the

**SERIAL NUMBER FACING UP**.

c. Feed the strap through the buckle and completely tighten.

The bracelet should be able to be rotated slightly, but not past the shin bone.

**Important Note** – To properly align the bracelet strap, ensure that the tooth alignment

tab is positioned between two teeth when the buckle is tightened. An “Open Strap

Detected” event will be generated if the strap is not properly aligned.

d. Tighten the retaining screws until the two sides of the buckle are flush.

**3. Finish with Direct Connect**

a. Open the Direct Connect application.

b. Log into the Direct Connect application using your SCRAMNET username and password.

**Connect Direct Connect Device with Your Computer**

To connect the Direct Connect device:

a. Plug the small (mini-B type) USB connector into the Direct Connect device.

b. Plug the large (A type) USB connector into a USB port on your computer.

The **red** and **blue** lights on the Direct Connect device blink for approximately 5 seconds

then both remain on.

Bracelet status in Direct Connect Application: *Waiting for Bracelet*

**Attach Direct Connect Device to SCRAM CAM Bracelet**

To attach the Direct Connect device:

a. Align the Direct Connect device with the top of the bracelet.

b. Slide the Direct Connect device down over the bracelet.

**Wake Up SCRAM CAM Bracelet**

To wake up the bracelet:

a. Momentarily place the magnet on the Direct Connect device where the word “magnet”

appears.

**Placing Magnet on Bracelet**

When magnet is placed on the Direct Connect device, the **red** light turns off while the **blue** light remains on.

Bracelet status in Direct Connect Application: *Communicating*

**At this time:**

1) The bracelet initialization process begins.

2) The initial alcohol reading is uploaded to SCRAMNET.

**When complete:**

-The **blue** light on the Direct Connect device turns off for approximately 10 seconds

then both lights turn back on.

-Bracelet status in Direct Connect Application: *Communication Complete*

**Note:** After 1 minute, the status changes to: *Waiting for Bracelet*

b. Remove the Direct Connect device from the bracelet.